IFC building model
Schema: "IFC4"
Description: "IFC Export"
File name: "KBS-10516403.ifc"
Time stamp: "2024-09-30T11:38:02"
Author: "Unknown"
Organization: "SWS SoftWare-Systeme GmbH"
Preprocessor: "SWS IFC Engine 2.1"
Originating system: "WinDelta PMS 2024"
Authorization: "Unknown Authorizer"
Application: "WinDelta PMS 2024" version "9.42d" identifier "www.sws-online.de" by Organization (no name given)

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application "WinDelta PMS 2024" version "9.42d" identifier "www.sws-online.de" by Organization (no name given) | change ADDED | created 1727696282 (2024-09-30T11:38:02Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "Data"
  IFCSITE "Site" | latitude 51° 42′ 6.487199″ | longitude 8° 46′ 0.8148″ | description "Description of Site"
    IFCBUILDING "Building" | description "Description of Building"
      IFCBUILDINGSTOREY "Building Storey" | elevation 0. | description "Description of Building Storey"
        IFCSPACE "Space" | description "Description of Space"
          contains 1 element
            1 x IFCELECTRICAPPLIANCE | names: "KBS-10516403" | descriptions: "ELEKTRO-NUDELKOCHER" | property sets: bSD_PSet_FoodServiceEquipmentIdentityData, bSD_PSet_FoodServiceEquipmentGeneral, bSD_PSet_FoodServiceEquipmentElectrical, bSD_PSet_FoodServiceEquipmentPlumbing, bSD_PSet_FoodServiceEquipmentPlumbing (2), bSD_PSet_FoodServiceEquipmentPlumbing (3)

Property sets
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Concealed = FALSE (IFCBOOLEAN)
    HandicapAccessible = TRUE (IFCBOOLEAN)
    MechanicalVentilationRate = 0 (IFCINTEGER)
    NaturalVentilation = TRUE (IFCBOOLEAN)
    NaturalVentilationRate = 0 (IFCINTEGER)
    OccupancyNumber = 0 (IFCINTEGER)
    OccupancyType = "" (IFCTEXT)
    PubliclyAccessible = TRUE (IFCBOOLEAN)
    Reference = "" (IFCTEXT)
  Pset_Draughting | properties | on 1 object (1 IFCSPACE)
    Color: Red = 0 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    Layer = "Rooms" (IFCLABEL)
  bSD_PSet_FoodServiceEquipmentIdentityData | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Description = "ELEKTRO-NUDELKOCHER" (IFCTEXT)
    Item Number = "KBS-10516403" (IFCTEXT)
    Manufacturer = "KBS" (IFCTEXT)
    Specification by Manufacturer = "TEIGWARENKOCHER" (IFCTEXT)
  bSD_PSet_FoodServiceEquipmentGeneral | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Depth Actual = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Actual = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Length Actual = 800. (IFCLENGTHMEASURE) [MILLI METRE]
  bSD_PSet_FoodServiceEquipmentElectrical | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Cycle = "50Hz" (IFCTEXT)
    Electric power = 17. (IFCREAL)
    Electrical Connection Height = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Electrical Connection X = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    Electrical Connection Y = 665. (IFCLENGTHMEASURE) [MILLI METRE]
    Electrical Remarks = "50Hz 3N" (IFCTEXT)
    Volts = "400V" (IFCTEXT)
  bSD_PSet_FoodServiceEquipmentPlumbing | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Cold Water Connection Height = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection X = 220. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection Y = 725. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Size = "3/4"" (IFCTEXT)
    Plumbing Remarks = "3/4"" (IFCTEXT)
  bSD_PSet_FoodServiceEquipmentPlumbing (2) | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Cold Water Connection Height (2) = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection X (2) = 620. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection Y (2) = 725. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Size (2) = "3/4"" (IFCTEXT)
    Plumbing Remarks (2) = "3/4"" (IFCTEXT)
  bSD_PSet_FoodServiceEquipmentPlumbing (3) | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Direct Waste Connection Height (3) = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Direct Waste Connection X (3) = 310. (IFCLENGTHMEASURE) [MILLI METRE]
    Direct Waste Connection Y (3) = 617. (IFCLENGTHMEASURE) [MILLI METRE]
    Direct Waste Size (3) = "1 1/4"" (IFCTEXT)
    Waste Remarks (3) = "1"" (IFCTEXT)
  bSD_PSet_FoodServiceEquipmentPlumbing (4) | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Direct Waste Connection Height (4) = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Direct Waste Connection X (4) = 710. (IFCLENGTHMEASURE) [MILLI METRE]
    Direct Waste Connection Y (4) = 617. (IFCLENGTHMEASURE) [MILLI METRE]
    Direct Waste Size (4) = "1 1/4"" (IFCTEXT)
    Waste Remarks (4) = "1"" (IFCTEXT)